RISK ASSESSMENT

Funday Entertainment Limited



RA - FUN014/15

|  |  |  |  |
| --- | --- | --- | --- |
| **LOCATION:** | Various Locations | **DATE:** | January 2015 |
| **OPERATION/PROCESS:** | Safe Use and Operation of the 6 Bed Trampoline Trailer |
| **HAZARDS IDENTIFIED:** | 1. Crush injuries from falling trailer sides,
2. Winch malfunction,
3. Equipment Collapse,
4. collision of persons on separate beds,
5. injuries from activities on the trampolines
 |
| **SECONDARY HAZARDS:** | Weather conditions, other people,  |
| **EXPOSED PERSONS:** | Staff, Members of the public using the trampolines. |
| **FREQUENCY OF EXPOSURE:** | As per Event Date/s | **DURATION OF EXPOSURE:** As per Event hours |
| ***RISK = LIKELIHOOD X SEVERITY*** |
| ***LIKELIHOOD*****0** = Zero to very low**1** = Very unlikely**2** = Unlikely | **3** = Likely**4** = Very likely**5** = Almost certain | ***SEVERITY*****0** = No injury or illness**1** = First aid injury or illness**2** = Minor injury or illness | **3** = “ 3 day “ injury or illness**4** = Major injury or illness **5** = Fatality, disablement injury, etc |
| **Risk Values:** LOW = **1 to 8** MEDIUM = **9 to 16** HIGH = **17 to 25** |
| **Activity Risk Rating:** *Likelihood* ***4*** *X Severity* ***5*** *= Total* ***20*** |
| **Activity Risk Value*:*** *LOW* *MEDIUM* ***HIGH***  |
| **CONTROL MEASURES** **Steps to be taken to avoid an accident or incident leading to an injury:** | 1. All equipment will be tested as and when required in accordance with the regulations including PAT testing of all electrical leads and Equipment. (Only required if flood lights are connected to a power source)
2. All equipment is to be inspected before being taken to an event or party. Any faults are to be reported immediately to the Funday Director.
3. Only a competent person is to set up and install the equipment ensuring the trampoline trailer is set up in accordance with the manufacturer’s instructions.
4. Only competent persons are to operate the battery powered winch system who have been authorised by the Company Director.
5. Ensure no unauthorised persons enter the area while the equipment is being set up or dismantled.
6. If power cables are installed for the flood lights the electric cable is to be checked on a regular basis to ensure they have not been moved/ tampered with and that all slip/ trip/ fall hazards are controlled and minimised.
7. All users are to be briefed on the safe methods of using the trampolines. Summersaults and jumping from one to another bed are the main activities that are banned.
8. All users are made aware of the picture boards showing the recommended and banned activities when using the trampolines.
9. All age groups are permitted to use the trampolines but as far as is reasonably practicable older and younger age groups will be kept separate.
10. Following an incident/ accident Funday staff are to inform the Funday Manager or client. All other trampoline beds will be cleared to prevent further risk of injury.
11. If powered by a generator a minimum of two Co2 fire extinguishers will be kept available at all times in case of emergencies and all staff will be trained on the correct use of them.
12. During poor weather the equipment will be closed to prevent slips and falls on the trampoline bed.
 |
| **Residual Risk Rating*:*** *Likelihood* ***2***  *X Severity* ***3***  *= Total* ***6*** |
| **MONITORING RESULTS:** | Event Manager / Director to ensure the above is adhered to for the risk to be acceptable |
| **REVIEW DATE:** | At regular intervals, not to exceed 12 months or when circumstances change. |
| **RESIDUAL RISK RATING: LOW** |
| **ASSESSOR:** | Andre Rayson | **POSITION:** | Senior Health & Safety Advisor |