Risk Assessment – 007 Laser Shooting Game Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, testing, supervised operation and dismantling of the 007 Laser Shooting Game for temporary hire at events. Players use infrared laser guns to aim at electronic targets in a controlled game area.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of equipment
	Staff
	Medium
	Use safe lifting techniques and transport aids.
	Low

	Electrical fault or damaged cables
	Staff/Public
	High
	PAT tested equipment, RCD protection and pre-use inspection.
	Low

	Trip hazards from cables
	All
	Medium
	Protect leads with cable covers and keep walkways clear.
	Low

	Unsafe aiming of laser guns
	Participants
	Medium
	Safety briefing; aim only at designated targets.
	Low

	Player collision while moving
	Participants
	Medium
	Clearly mark playing positions and supervise activity.
	Low

	Equipment malfunction
	All
	Medium
	Function test before each hire; isolate faulty equipment.
	Low

	Unauthorised access to play area
	Public
	Medium
	Maintain barriers and operator control.
	Low



Operational Controls
Set up the attraction on a firm, level surface with a clearly defined shooting area and safe spectator zone.
Test all laser guns, electronic targets, scoring systems and sound effects before opening.
Protect and secure all power leads using cable covers and keep them away from player movement areas.
Allow only the manufacturer's recommended number of players to participate at one time.
Brief players to aim only at designated electronic targets and never at other people.
Players must remain within the designated shooting position unless instructed otherwise.
Maintain continuous operator supervision throughout play.
Stop the game immediately if unsafe behaviour, damaged equipment or faults are identified.
Emergency Procedures
Stop the game immediately if unsafe behaviour, damaged equipment or faults are identified.
Isolate the electrical supply before inspecting the equipment.
Provide first aid and contact emergency services if required.
Remove defective equipment from service until repaired.
Record all accidents, incidents and near misses.
Inspection Checklist
Cabinet stable and level.
Laser guns and triggers operate correctly.
Targets, sensors and scoring display operate correctly.
Power cable and plug undamaged.
PAT label current where applicable.
No loose fixings, exposed wiring or sharp edges.
Playing area free from slip and trip hazards.
Training Requirements
Safe delivery, installation and dismantling.
Manual handling techniques.
Electrical safety and cable management.
Pre-use inspections and functional testing.
Participant briefing and supervision.
Emergency isolation and accident reporting.
