Risk Assessment – 360 Photo Booth Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of an indoor archery stall using low-poundage bows and suction-cup or foam safety arrows for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure platform, camera arm and components during transport and setup.
	Low

	Participant falls from rotating platform
	Participants
	High
	Provide clear instructions before use; ensure participants remain centrally positioned; limit numbers/weight to manufacturer guidance; supervise continuously.
	Low

	Participant loses balance while platform rotates
	Participants
	High
	Require suitable footwear and controlled movement; prohibit running, jumping or unsafe dancing; stop rotation immediately if a participant becomes unstable.
	Low

	Collision with camera arm / moving equipment
	Participants
	High
	Maintain a defined operating zone; keep participants clear of the camera arm and moving mechanism; supervise every session.
	Low

	Hair, clothing or accessories becoming caught
	Participants
	High
	Secure loose hair, clothing, scarves and accessories before operation; prohibit loose items near the rotating mechanism; stop equipment before intervention.
	Low

	Finger or hand trapping in moving mechanism
	Participants/Staff
	High
	Keep hands clear of moving parts and pinch points; never reach toward the mechanism while operating; isolate power before maintenance.
	Low

	Participant falls from or steps off platform incorrectly
	Participants
	High
	Ensure platform access is clear; instruct users when to enter and exit; stop the platform before participants leave where applicable; supervise continuously.
	Low

	Electrical equipment / cable hazard
	Participants/Staff
	Medium
	Inspect power supply, plugs and cables before use; route cables safely away from walkways; isolate defective equipment.
	Low

	Trips around platform, cables or equipment
	All
	Medium
	Keep the operating area clear of bags, props and cables; secure or route cables away from pedestrian routes; maintain good housekeeping.
	Low

	Unstable or unsuitable installation
	Participants/Spectators
	High
	Position the booth on a suitable, stable and level surface; ensure platform and equipment are secure before operation.
	Low

	Overcrowding on platform or around booth
	Participants/Spectators
	High
	Control participant numbers according to manufacturer guidance; maintain a clear spectator area and supervise queues.
	Low

	Props or accessories becoming projectiles / trip hazards
	Participants/Spectators
	Medium
	Use only suitable props; inspect before use; remove damaged or unsuitable props; keep unused items outside the operating area.
	Low

	Damaged platform, camera arm or components
	All
	High
	Inspect all structural and moving components before each session; remove damaged equipment from use immediately.
	Low

	Poor lighting / visibility
	Participants/Staff
	Medium
	Provide adequate ambient lighting so the platform, camera arm, controls, cables and surrounding hazards are clearly visible.
	Low

	Participant behaviour / excessive movement
	Participants
	High
	Give a clear safety briefing; prohibit climbing, pushing, jumping onto the platform or deliberate interference; stop use if behaviour becomes unsafe.
	Low

	Emergency access obstructed
	All
	Medium
	Position the booth so emergency routes, exits and venue access remain clear at all times.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Follow manufacturer guidance; assess participant suitability and provide appropriate supervision, particularly for children and vulnerable users.
	Low

	Equipment movement during rotation / mechanical fault
	Participants/Staff
	High
	Complete pre-use checks; operate only with guards and components correctly fitted; stop immediately if unusual noise, movement or mechanical fault occurs.
	Low


Operational Controls
 Set up on a suitable, stable and level surface with adequate clearance around the 360 Photo Booth.
 Give every participant a clear safety briefing before use, including safe entry, exit and movement on the rotating platform.
 Keep participant numbers, weight and platform use within manufacturer requirements and maintain continuous supervision.
 Secure loose hair, clothing, scarves and accessories and ensure props do not create additional hazards.
 Stop activity immediately if a participant becomes unstable, unsafe behaviour occurs, equipment faults develop or the operating area becomes unsafe.
Emergency Procedures
 Stop the 360 Photo Booth immediately following any incident.
 Provide first aid where required and contact emergency services if necessary.
 Isolate damaged or defective equipment and prevent further use.
 Record all accidents and near misses.
Inspection Checklist
 Platform and frame free from damage.
 Rotating mechanism operates smoothly and correctly.
 Camera arm and mounting secure and undamaged.
 Safety guards and protective components correctly fitted where applicable.
 Controls and emergency stop function correctly where fitted.
Training Requirements
 Staff trained in safe 360 Photo Booth operation, manual handling, participant briefing, supervision, moving-part hazards, emergency procedures and equipment inspection.
