Risk Assessment – Bouncy Castle
Persons Involved: Site team
Also Present: Venue staff, Guests
Equipment: Portable inflatable bouncy castle with blower, anchor stakes/sandbags, safety mats and RCD-protected extension leads.
Location: Various Locations
	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Over-enthusiastic users
	Supervise at all times. No flips, wrestling or climbing walls.
	1
	3
	3
	Monitor during busy periods.

	Mixed ages/sizes
	Separate users by age/size.
	1
	3
	3
	Display age limits.

	Adverse weather
	Do not operate in high winds, heavy rain or thunderstorms.
	1
	5
	5
	Monitor weather.

	Falls
	Safety mats fitted. Fully inflate before use.
	2
	3
	6
	Check landing area.

	Lack of supervision
	Trained operator present at all times.
	1
	5
	5
	Never leave unattended.

	Trip hazards
	Secure cables and anchor points.
	1
	2
	2
	Barrier cables if needed.

	Incorrect positioning
	Install on level ground with clearances.
	1
	4
	4
	Site inspection.

	Overcrowding
	Do not exceed manufacturer capacity.
	2
	3
	6
	Control queue.

	Choking
	No food, drink or chewing gum.
	1
	4
	4
	Display rules.

	Loose items
	Remove shoes, glasses and jewellery.
	1
	4
	4
	Operator checks users.

	Fire
	No smoking or naked flames nearby.
	1
	5
	5
	Extinguisher available.

	Spectators
	Keep entrance/exit clear.
	2
	2
	4
	Queue barriers.

	Emergency
	Stop use, call 999 if serious.
	N/A
	N/A
	N/A
	First aid available.

	Alcohol/drugs
	Refuse intoxicated users.
	1
	3
	3
	Operator discretion.

	Inflation/deflation
	No users during inflation/deflation.
	1
	5
	5
	Only trained staff.

	Anchorage
	Use approved anchors/ballast and inspect regularly.
	1
	5
	5
	Recheck throughout event.



