Risk Assessment – Bungee Run Hire
Activity: Hire and supervised operation of an inflatable Bungee Run.
Equipment: Inflatable, blower(s), anchors, harnesses, bungee cords, RCD.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Strains
	Team lift; trolley
	Low

	Incorrect installation
	Users
	Collapse
	Install per manufacturer guidance
	Low

	Poor anchoring
	Users
	Movement
	Secure stakes/ballast; inspect
	Low

	Electrical blower
	All
	Shock/trips
	PAT, RCD, cable covers
	Low

	Trips entering/exiting
	Users
	Falls
	Supervise access
	Low

	Participant collisions
	Users
	Bruises
	One per lane; supervision
	Medium

	Bungee recoil
	Users
	Impact
	Harness checked before use
	Medium

	Falls while running
	Users
	Sprains
	Clear briefing; suitable surface
	Medium

	Horseplay
	Users
	Injury
	Stop misuse immediately
	Medium

	Weather
	Users
	Instability
	Do not use in high winds
	Low

	Damaged equipment
	Users
	Injury
	Inspect before hire
	Low


Additional Control Measures
Continuous supervision.
Remove shoes, jewellery and sharp objects.
Observe age/weight limits.
Inspect before every hire.
Emergency Procedures
Stop activity, isolate power if required, administer first aid, record incidents and remove defective equipment from service.
