Risk Assessment – Bungee Trampolines Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of bungee trampoline equipment for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	Medium
	Use safe lifting techniques/team lifts; secure trampoline, frame, harnesses, bungees and accessories during transport/setup.
	Low

	Frame instability
	Participants/Spectators
	High
	Set up on suitable firm, level ground; assemble and stabilise as specified; inspect before use.
	Low

	Participant fall / uncontrolled jump
	Participants
	High
	Follow manufacturer instructions; use approved harness/bungee system; control one participant at a time; competent supervision.
	Low

	Harness / bungee failure
	Participants
	High
	Pre-use inspection of harnesses, bungees, ropes, connectors and attachment points; use approved components only; remove defects from service.
	Low

	Unsuitable participant size/ability
	Participants
	High
	Apply manufacturer's age, height and weight limits; assess suitability before use; do not exceed capacity.
	Low

	Collision with frame/equipment
	Participants
	High
	Maintain adequate clearance; give clear instructions; prohibit contact with frame and unsafe manoeuvres.
	Low

	Incorrect use / misuse
	Participants
	High
	Safety briefing; prohibit unauthorised flips, twisting, swinging, climbing or interference with harness/bungees.
	Low

	Collision / entanglement
	Participants
	High
	Use approved spacing and operating system; normally one participant per jumping position; continuous supervision.
	Low

	Trips/slips around attraction
	All
	Medium
	Keep access and landing areas clear, clean and dry; manage queues and loose equipment.
	Low

	Damaged trampoline/frame
	Participants/Staff
	High
	Inspect frame, mat, springs, padding and fixings before each use; remove damaged equipment from service.
	Low

	Overcrowding / spectators
	Participants/Spectators
	Medium
	Control queues and participant numbers; maintain exclusion zones around the attraction.
	Low

	Weather conditions
	All
	High
	Follow manufacturer's weather/wind limits; secure correctly; stop operation in unsuitable conditions.
	Low

	Emergency access
	All
	Medium
	Keep emergency routes, exits and venue access clear.
	Low

	Electrical/ancillary equipment
	Staff/Participants
	Medium
	Inspect electrical equipment where used; route cables safely and protect connections from water/damage.
	Low


Operational Controls
Set up on suitable firm, level ground with adequate clearance and access.
Inspect frame, trampoline, harnesses, bungees, attachment points and fixings before each use.
Check participant age, height, weight and suitability before fitting the harness.
Fit and check the harness correctly and give a clear safety briefing.
Maintain competent active supervision and control participant numbers.
Stop immediately if equipment is damaged, a participant is distressed, weather deteriorates or any unsafe condition develops.
Emergency Procedures
Stop the attraction following any incident or unsafe condition.
Assist/lower the participant safely in accordance with the manufacturer's emergency procedure.
Provide first aid where required and contact emergency services if necessary.
Remove defective equipment from service and record accidents and near misses.
Inspection Checklist
Frame, trampoline, mat, padding and structural components secure and undamaged.
Harnesses, bungees, ropes, connectors and attachment points inspected and secure.
Fixings, anchoring/stabilisation and safety components checked.
Activity/landing areas clear; emergency routes unobstructed.
Participant limits, supervision and operating restrictions established.
Training Requirements
Staff trained in Bungee Trampoline operation, inspection, harness fitting, participant briefing, supervision, emergency procedures, weather limits and incident response.
