Risk Assessment – Catch It Reaction Game Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, testing, supervised operation and dismantling of the Catch It Reaction Game for temporary hire at events. The game uses illuminated electronic reaction pads that players strike with their hands to achieve the fastest score.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of equipment
	Staff
	Medium
	Use two-person lifts and suitable transport equipment.
	Low

	Electrical fault or damaged cables
	Staff/Public
	High
	PAT tested, RCD protection, visual inspection before use.
	Low

	Trip hazards from cables
	All
	Medium
	Protect leads with cable covers and route away from walkways.
	Low

	Player collision during rapid movement
	Participants
	Medium
	Provide 1.5 m clear play area and supervise play.
	Low

	Impact injuries to hands/fingers
	Participants
	Medium
	Use only open hands on reaction pads; safety briefing before play.
	Low

	Equipment movement
	Participants
	Medium
	Install on a firm, level surface.
	Low

	Equipment malfunction
	All
	Medium
	Function test before each hire; isolate faulty equipment.
	Low



Operational Controls
Position the Catch It Reaction Game on a firm, level surface with a minimum 1.5 metre clear playing area around all sides.
Complete a full functional test of all illuminated touch pads, timers, scoring displays and sound effects before use.
Ensure all electrical leads are protected using cable covers and routed away from pedestrian routes.
Allow only the recommended number of players at any one time.
Instruct participants to strike only the illuminated reaction pads using open hands.
Players must remain within the designated playing position throughout the game.
Maintain continuous adult supervision during operation.
Stop the game immediately if unsafe behaviour or equipment faults are identified.
Emergency Procedures
Stop the game immediately following any accident or equipment fault.
Isolate the electrical supply before inspecting the equipment.
Provide first aid and contact emergency services if required.
Remove defective equipment from service until repaired.
Record all accidents, incidents and near misses.
Inspection Checklist
Cabinet stable and level.
Reaction pads respond correctly.
Lights, timer and scoring display operational.
Power cable and plug undamaged.
PAT label current where applicable.
No loose fixings, exposed wiring or sharp edges.
Playing area free from slip and trip hazards.
Training Requirements
Safe delivery, installation and dismantling.
Manual handling techniques.
Electrical safety and cable management.
Pre-use inspections and functional testing.
Participant briefing and supervision.
Emergency isolation and accident reporting.
