Risk Assessment – Inflatable Demolition Wrecking Ball Hire
Activity: Hire and supervised operation of an inflatable demolition wrecking ball game.
Equipment: Inflatable game, blower(s), RCD-protected power supply, anchors/ballast, suspended foam wrecking ball, safety mats.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Back strains/crush injuries
	Team lifting and use of handling aids
	Low

	Incorrect installation
	Users, Staff
	Collapse/instability
	Installed by trained staff to manufacturer guidance
	Low

	Poor anchoring
	Users
	Inflatable movement
	Secure with stakes or ballast; inspect regularly
	Low

	Electrical blower/cables
	All
	Electric shock or trips
	PAT tested blower, RCD, cable covers
	Low

	Falls from podium
	Participants
	Bruises/sprains
	Safety briefing, supervise users, cushioned inflatable surface
	Medium

	Impact from wrecking ball
	Participants
	Minor injuries
	Use foam ball only, enforce safe play rules
	Medium

	Collisions between participants
	Participants
	Bruises
	Maximum 4 users; supervise continuously
	Medium

	Horseplay
	Participants
	Injury
	No pushing, climbing or misuse
	Medium

	Adverse weather
	Users
	Instability
	Cease operation in high winds/heavy rain
	Low

	Damaged equipment
	Users
	Injury
	Inspect before each hire and remove defective equipment
	Low

	Blocked fire exits
	Public
	Delayed evacuation
	Position away from emergency exits
	Low


Additional Control Measures
Continuous trained operator or responsible adult supervision.
Remove shoes, jewellery and sharp objects before use.
Observe manufacturer age, height and weight limits.
No food or drink on the inflatable.
Daily pre-use inspection before operation.
Emergency Procedures
Stop play immediately if equipment becomes unsafe or weather deteriorates. Switch off blower if required, administer first aid, record all incidents and remove defective equipment from service.
