Risk Assessment – Disco Dome Hire
Activity: Hire and supervised operation of an inflatable Disco Dome.
Equipment: Inflatable Disco Dome, blower, anchors/ballast, PAT-tested sound and lighting system, RCD, extension leads.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Back strain/crush injuries
	Team lift and handling aids
	Low

	Incorrect installation
	Users, Staff
	Collapse/instability
	Setup by trained staff to manufacturer instructions
	Low

	Poor anchoring
	Users
	Inflatable movement
	Stake/ballast correctly and inspect
	Low

	Electrical equipment
	All
	Electric shock
	PAT tested, RCD protection, visual checks
	Low

	Trailing cables
	Public
	Trips
	Cable covers and safe routing
	Low

	Slips, trips and falls
	Participants
	Bruises/sprains
	Keep entrance clear and supervise
	Medium

	Collisions inside inflatable
	Participants
	Minor injuries
	Limit user numbers and separate ages where practical
	Medium

	Horseplay
	Participants
	Injury
	No climbing, pushing or somersaults
	Medium

	High sound levels
	Users
	Hearing discomfort
	Maintain appropriate volume
	Low

	Lighting effects
	Users
	Discomfort
	Warn users of flashing lights; do not use if unsuitable
	Low

	Adverse weather
	Users
	Instability
	Stop use in high winds/heavy rain
	Low

	Damaged equipment
	Users
	Injury
	Inspect before each hire
	Low

	Blocked fire exits
	Public
	Delayed evacuation
	Keep escape routes clear
	Low


Additional Control Measures
Continuous adult/operator supervision.
Remove shoes, jewellery and sharp objects.
No food or drink inside the inflatable.
Observe manufacturer age, height and weight limits.
Complete daily pre-use inspection.
Emergency Procedures
Stop play immediately if equipment becomes unsafe or weather deteriorates. Isolate electrical power if required, administer first aid, record incidents and remove defective equipment from service.
