Risk Assessment – Ice Cube Ski Blizzard Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of an indoor archery stall using low-poundage bows and suction-cup or foam safety arrows for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure components during transport and setup; use suitable handling equipment where necessary.
	Low

	Participant falls while using ski simulator
	Participants
	High
	Provide a clear safety briefing and demonstration; ensure participants use the equipment correctly; maintain continuous supervision; stop use if balance or control is lost.
	Low

	Participant loses balance during simulated skiing
	Participants
	High
	Allow only suitable participants; provide adequate space around the unit; instruct users to maintain controlled movements; stop the activity if unsafe movement occurs.
	Low

	Collision with equipment or surrounding objects
	Participants/Spectators
	High
	Maintain a clear operating area around the simulator; prevent spectators entering the active zone; supervise continuously.
	Low

	Participant overexertion or fatigue
	Participants
	Medium
	Provide controlled sessions and rest periods; encourage participants to stop if tired, dizzy or uncomfortable; supervise throughout.
	Low

	Finger or hand trapping in moving components
	Participants/Staff
	Medium
	Keep hands clear of moving mechanisms and pinch points; do not interfere with the equipment while operating; isolate before maintenance.
	Low

	Electrical equipment / cable hazard
	Participants/Staff
	Medium
	Inspect power supply, plugs and cables before use; route cables safely away from walkways; isolate defective equipment.
	Low

	Trips around equipment and cables
	All
	Medium
	Keep the surrounding floor clear of cables, bags and other equipment; maintain good housekeeping.
	Low

	Damaged ski simulator, controls or components
	All
	High
	Inspect the simulator, controls, skis and associated components before each session; remove damaged equipment from use.
	Low

	Unstable or unsuitable installation
	Participants/Spectators
	High
	Position the equipment on a suitable, stable and level surface; ensure it is securely installed before operation.
	Low

	Spectators entering operating area
	Public
	Medium
	Clearly define the operating area and keep spectators outside the active zone while the simulator is in use.
	Low

	Overcrowding around simulator
	Participants/Spectators
	Medium
	Control participant numbers and queues; maintain adequate clearance around the equipment; supervise waiting participants.
	Low

	Incorrect use / deliberate misuse
	Participants
	High
	Give a clear demonstration and safety briefing; prohibit climbing, jumping onto or tampering with the equipment; stop unsafe behaviour.
	Low

	Poor lighting / visibility
	Participants/Staff
	Medium
	Provide adequate lighting so the simulator, controls, cables and surrounding hazards are clearly visible.
	Low

	Emergency access obstructed
	All
	Medium
	Position the equipment so exits, emergency routes and venue access remain clear at all times.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Follow manufacturer guidance where available; assess participant suitability and provide appropriate supervision.
	Low


Operational Controls
 Set up on a suitable, stable and level surface with adequate clearance around the Ice Cube Ski Blizzard.
 Give every participant a clear safety briefing and demonstration before use.
 Assess participant suitability and ensure users understand how to maintain controlled movements while operating the simulator.
 Maintain continuous adult supervision and keep spectators outside the active operating area.
 Stop activity immediately if a participant loses control, unsafe behaviour occurs, equipment becomes unstable or any fault is identified.
Emergency Procedures
 Stop the Ice Cube Ski Blizzard immediately following any incident.
 Provide first aid where required and contact emergency services if necessary.
 Isolate damaged or defective equipment and prevent further use.
 Record all accidents and near misses.
Inspection Checklist
 Simulator structure and frame free from damage.
 Skiing surface and moving components secure and functioning correctly.
 Controls and operating mechanisms functioning correctly.
 Skis, footwear/interface and associated components free from damage.
 Electrical supply, plug and cables free from visible damage where applicable.
Training Requirements
 Staff trained in safe Ice Cube Ski Blizzard operation, manual handling, participant briefing, supervision, emergency procedures and equipment inspection.
