Risk Assessment – Basketball Shooting Game (Public Hire)
Persons Involved: Site Team / Trained Operators
Also Present: Members of the Public, Venue Staff
Equipment: Inflatable basketball game, blower, anchor stakes/sandbags, RCD, extension leads, basketballs
Location: Various Public Event Locations

	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Manual handling
	Team lifts and correct handling techniques.
	1
	3
	3
	Staff training.

	Installation
	Installed by trained staff following manufacturer instructions.
	1
	5
	5
	Pre-opening inspection.

	Anchoring
	All anchor points secured using stakes or ballast to manufacturer specification.
	1
	5
	5
	Check throughout event.

	Blower failure
	Continuous blower operation monitored. Game closed immediately if blower stops.
	1
	5
	5
	Inspect blower and power before reopening.

	Inflation/Deflation
	No users permitted during inflation or deflation.
	1
	5
	5
	Operator control only.

	Wind & Weather
	Do not operate in winds exceeding manufacturer limits (typically 24 mph / 38 km/h). Close during thunderstorms or heavy rain.
	1
	5
	5
	Monitor weather continuously.

	Trip hazards
	Secure electrical leads and keep playing area clear.
	1
	2
	2
	Routine inspections.

	Ball strikes
	Safety netting fitted where applicable.
	2
	2
	4
	Operator supervision.

	Misuse
	No climbing or rough play.
	2
	3
	6
	Display safety rules.

	Electrical safety
	PAT-tested blower, RCD protection, cables protected.
	1
	5
	5
	Daily inspection.

	Emergency
	Stop use immediately if unsafe; first aid available; call 999 if required.
	1
	5
	5
	Record incidents and quarantine faulty equipment.

	HSE compliance
	Operate in accordance with HSE guidance and manufacturer operating manual.
	1
	4
	4
	Annual review and staff refresher training.



