Risk Assessment – Inflatable Connect 4 Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of inflatable connect 4 equipment for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of inflatable and equipment
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure inflatable, game pieces and blower during transport and setup.
	Low

	Inflatable instability / inadequate anchoring
	Participants/Spectators
	High
	Set up on suitable firm, level ground; use specified anchoring; inspect before use and stop if movement occurs.
	Low

	Game pieces falling / striking participant
	Participants/Spectators
	Medium
	Ensure pieces are handled as intended; prohibit throwing pieces; supervise younger participants.
	Low

	Trips from game pieces / equipment
	All
	Medium
	Keep loose pieces in a designated area; collect dropped items promptly; maintain clear walkways.
	Low

	Climbing / leaning on inflatable
	Participants
	Medium
	Provide clear instructions; prohibit climbing, hanging or leaning on unsuitable sections; supervise use.
	Low

	Incorrect use / deliberate misuse
	Participants
	Medium
	Provide a safety briefing; prohibit throwing pieces, pushing, rough play and unsafe behaviour.
	Low

	Damaged inflatable / game pieces
	All
	Medium
	Inspect inflatable and all game components before each session; remove damaged equipment from service.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Provide clear instructions and appropriate supervision; consider age, size, mobility and ability.
	Low

	Overcrowding around game
	Participants/Spectators
	Medium
	Control player numbers and queues; maintain a clearly defined playing and spectator area.
	Low

	Electrical equipment / blower
	Staff/Participants
	High
	Inspect blower and connections; route cables safely; keep electrical connections dry.
	Low

	Emergency access obstructed
	All
	Medium
	Position the game so emergency routes and exits remain clear at all times.
	Low


Operational Controls
Set up the Inflatable Connect 4 activity on suitable ground/surface with adequate clearance and access.
Inspect equipment before each use and provide a clear safety briefing before participation.
Control participant numbers and maintain clearly defined playing, access and spectator areas.
Prohibit running, pushing, climbing, deliberate misuse and other unsafe behaviour.
Follow manufacturer operating, participant, anchoring and weather requirements where applicable.
Stop the activity immediately if equipment is damaged, unstable or conditions become unsafe.
Emergency Procedures
Stop the Inflatable Connect 4 activity immediately following any incident or unsafe condition.
Ensure participants leave the active area safely and keep emergency routes clear.
Provide first aid where required and contact emergency services if necessary.
Remove damaged equipment from service and record all accidents and near misses.
Inspection Checklist
Equipment structure and components stable, secure and free from damage.
Activity surface, access and landing areas clean and free from defects or trip hazards.
Access, exit and spectator areas clearly defined.
Emergency routes and venue access remain clear.
Participant capacity, supervision and restrictions clearly established.
Training Requirements
Staff trained in safe Inflatable Connect 4 operation, equipment inspection, participant briefing, supervision, crowd/access control, emergency procedures and incident response.
