Risk Assessment – Inflatable Play Park Hire
Activity: Hire and supervised operation of inflatable play parks.
Equipment: Inflatable play park, blowers, anchors/ballast, RCD, mats.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Strains
	Team lift/manual handling
	Low

	Incorrect installation
	Users
	Collapse
	Install to manufacturer instructions
	Low

	Poor anchoring
	Users
	Movement
	Stake/ballast correctly; inspect
	Low

	Electrical equipment
	All
	Shock/trips
	PAT, RCD, cable covers
	Low

	Entry/exit trips
	Users
	Falls
	Mats and supervised access
	Low

	Falls inside
	Children
	Bruises
	Supervision; no overcrowding
	Medium

	User collisions
	Children
	Minor injuries
	Separate ages/sizes
	Medium

	Horseplay
	Users
	Injury
	Enforce rules
	Medium

	Adverse weather
	Users
	Instability
	Stop use in high winds/rain
	Low

	Damaged equipment
	Users
	Injury
	Inspect before hire
	Low

	Blocked fire exits
	Public
	Evacuation delay
	Keep exits clear
	Low


Additional Control Measures
Continuous supervision.
Remove shoes and sharp objects.
No food or drink.
Observe age/weight limits.
Level ground only.
Emergency Procedures
Stop play immediately if unsafe. Isolate power if required, provide first aid, record incidents and remove defective equipment from service.
