Risk Assessment – Inflatable Side Stalls Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of inflatable side stalls equipment for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of inflatable and equipment
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure inflatable, blower and stall equipment during transport and setup.
	Low

	Inflatable instability / inadequate anchoring
	Participants/Spectators
	High
	Set up on suitable firm, level ground; use specified anchoring; inspect before use and stop if movement occurs.
	Low

	Deflation / loss of pressure
	Participants/Spectators
	High
	Use correct blower and connections; maintain inflation as required; stop use if pressure is lost.
	Low

	Trips, slips and falls
	All
	Medium
	Operate on a clean, dry and level surface; keep customer and staff routes clear; remove hazards promptly.
	Low

	Stall equipment striking / falling
	Participants/Staff
	Medium
	Secure counters, signage and accessories; do not overload surfaces; inspect before opening.
	Low

	Incorrect use / deliberate misuse
	Participants
	Medium
	Provide clear instructions; prohibit climbing, leaning on unsuitable parts, throwing equipment or unsafe behaviour.
	Low

	Damaged inflatable / stall components
	All
	High
	Inspect inflatable, counters, fixtures and accessories before each session; remove damaged items from service.
	Low

	Electrical equipment / blower
	Staff/Participants
	High
	Use suitable electrical equipment and protection; route cables safely; keep connections dry; inspect before use.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Provide appropriate supervision and consider participant age, mobility and ability where activities are provided.
	Low

	Overcrowding / queue management
	Participants/Spectators
	Medium
	Control queues and numbers; maintain a clearly defined customer and staff area.
	Low

	Emergency access obstructed
	All
	Medium
	Position the stall so emergency routes, exits and venue access remain clear.
	Low

	Weather conditions
	All
	High
	For outdoor use, follow manufacturer's weather limits; secure appropriately and stop use in unsuitable conditions.
	Low


Operational Controls
Set up the Inflatable Side Stalls activity on suitable ground/surface with adequate clearance and access.
Inspect equipment before each use and provide a clear safety briefing before participation.
Control participant numbers and maintain clearly defined playing, access and spectator areas.
Prohibit running, pushing, climbing, deliberate misuse and other unsafe behaviour.
Follow manufacturer operating, participant, anchoring and weather requirements where applicable.
Stop the activity immediately if equipment is damaged, unstable or conditions become unsafe.
Emergency Procedures
Stop the Inflatable Side Stalls activity immediately following any incident or unsafe condition.
Ensure participants leave the active area safely and keep emergency routes clear.
Provide first aid where required and contact emergency services if necessary.
Remove damaged equipment from service and record all accidents and near misses.
Inspection Checklist
Equipment structure and components stable, secure and free from damage.
Activity surface clean and free from defects or trip hazards.
Access, exit and spectator areas clearly defined.
Emergency routes and venue access remain clear.
Participant capacity, supervision and restrictions clearly established.
Training Requirements
Staff trained in safe Inflatable Side Stalls operation, equipment inspection, participant briefing, supervision, crowd/access control, emergency procedures and incident response.
