Risk Assessment – Inflatable Slide
Persons Involved: Site Team
Also Present: Venue Staff, Guests
Equipment: Portable inflatable slide with blower, anchor stakes/sandbags, safety mats and RCD-protected extension leads.
Location: Various Locations
	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Manual handling
	Use team lifts and correct lifting techniques.
	1
	3
	3
	Staff training.

	Trip hazards
	Secure cables and keep access routes clear.
	1
	2
	2
	Barrier if required.

	Mixed ages/sizes
	Separate users by age and size.
	1
	3
	3
	Monitor continuously.

	Climbing the slide
	Users climb steps only; no climbing up slide.
	2
	3
	6
	Operator supervision.

	Rough play
	No pushing, wrestling or somersaults.
	2
	3
	6
	Remove offenders.

	Falls from slide
	Safety mats at exit; clear landing area.
	2
	4
	8
	Supervise landing zone.

	Overcrowding
	One user per lane unless manufacturer states otherwise.
	2
	3
	6
	Control queue.

	Weather
	Do not use in high winds, heavy rain or thunderstorms.
	1
	5
	5
	Monitor weather.

	Electrical
	PAT-tested blower with RCD protection.
	1
	5
	5
	Inspect before use.

	Loose items
	Remove shoes, glasses and jewellery.
	1
	4
	4
	Operator checks users.

	Food/drinks
	No food, drinks or chewing gum.
	1
	4
	4
	Display signage.

	Fire
	No smoking or naked flames nearby.
	1
	5
	5
	Fire extinguisher available.

	Unauthorised use
	Deflate and secure when unattended.
	1
	3
	3
	Switch off blower.

	Inflation/deflation
	No users during inflation or deflation.
	1
	5
	5
	Trained staff only.

	Anchorage
	Use approved anchors/ballast and inspect regularly.
	1
	5
	5
	Recheck throughout event.

	Emergency
	Stop use immediately if serious injury occurs; call 999 if required.
	N/A
	N/A
	N/A
	First aid available.



