Risk Assessment – Mega Buzzer Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of an indoor archery stall using low-poundage bows and suction-cup or foam safety arrows for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure the unit and components during transport and setup.
	Low

	Participant contact with buzzer/game unit
	Participants
	Medium
	Use the buzzer only as designed; provide clear instructions; prohibit climbing, leaning or striking the unit; supervise use.
	Low

	Finger or hand trapping around buzzer/control
	Participants
	Medium
	Keep fingers clear of gaps and edges; do not interfere with internal or moving components; inspect the control before use.
	Low

	Electrical equipment / cable hazard
	Participants/Staff
	Medium
	Inspect power supply, plugs and cables before use; route cables safely away from walkways; isolate defective equipment.
	Low

	Trips around equipment and cables
	All
	Medium
	Keep the floor clear of cables, bags and other equipment; route cables away from pedestrian routes and maintain good housekeeping.
	Low

	Damaged buzzer, housing or display
	All
	Medium
	Inspect the buzzer, housing, display and associated components before each session; remove damaged equipment from use.
	Low

	Incorrect use / deliberate misuse
	Participants
	Medium
	Give a clear demonstration and safety briefing; prohibit striking, kicking, climbing on or tampering with the equipment.
	Low

	Competitive behaviour / participant collision
	Participants
	Medium
	Set clear rules before play; control player positions and movement; prohibit pushing or unsafe behaviour; supervise continuously.
	Low

	Overcrowding around game
	Participants/Spectators
	Medium
	Control player numbers and queues; maintain a clear operating and spectator area.
	Low

	Spectators interfering with controls
	Public
	Medium
	Define the operating area and keep spectators clear of the buzzer and controls while the game is active.
	Low

	Slips or falls
	All
	Medium
	Operate on a clean, dry and level surface; keep the surrounding floor clear of loose objects and trip hazards.
	Low

	Poor lighting / visibility
	Participants/Staff
	Medium
	Provide adequate lighting so the buzzer, display, cables and surrounding hazards are clearly visible.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Follow manufacturer or event guidance where available; provide clear instructions and appropriate supervision, particularly for children.
	Low

	Emergency access obstructed
	All
	Medium
	Position the game so emergency routes, exits and venue access remain clear at all times.
	Low

	Participant frustration or overexertion
	Participants
	Low
	Keep play controlled; allow reasonable breaks; stop activity if a participant becomes distressed, fatigued or unwell.
	Low


Operational Controls
 Set up on a suitable, stable and level surface with adequate clearance around the Mega Buzzer.
 Give participants a clear safety briefing covering correct use of the buzzer, game rules and prohibited behaviour.
 Maintain continuous supervision and control player numbers, positions and queues.
 Keep spectators outside the immediate operating area and prevent interference with the controls.
 Stop activity immediately if equipment becomes damaged, unsafe behaviour occurs, an electrical fault develops or the operating area becomes unsafe.
Emergency Procedures
 Stop the Mega Buzzer immediately following any incident.
 Provide first aid where required and contact emergency services if necessary.
 Isolate damaged or defective equipment and prevent further use.
 Record all accidents and near misses.
Inspection Checklist
 Buzzer housing and game structure free from damage.
 Buzzer/control secure and functioning correctly.
 Display, lights or sound functions operate correctly where fitted.
 Electrical supply, plug and cables free from visible damage where applicable.
 Unit stable and securely positioned.
Training Requirements
 Staff trained in safe Mega Buzzer operation, manual handling, customer briefing, participant supervision, emergency procedures and equipment inspection.
