Risk Assessment – Photo Booth
Persons Involved: Site Team
Also Present: Staff, Customers, Visitors
Equipment: Portable photo booth with camera, lighting, printer, backdrop, props, electrical equipment and RCD-protected extension leads.
Location: Various Locations
	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Manual handling
	Use safe lifting techniques when transporting and assembling equipment.
	1
	3
	3
	Staff training.

	Trip hazards
	Secure cables and keep access routes clear.
	1
	2
	2
	Routine inspections.

	Electrical safety
	PAT-tested equipment connected via RCD protection.
	1
	5
	5
	Pre-use checks.

	Equipment instability
	Ensure booth, backdrop and lighting are securely assembled.
	1
	4
	4
	Inspect before use.

	Crowding
	Manage queues and prevent overcrowding around the booth.
	2
	3
	6
	Use barriers if required.

	Slips
	Clean spillages immediately and keep floor clear.
	2
	3
	6
	Housekeeping.

	Props misuse
	Provide safe props only; no sharp or hazardous items.
	1
	3
	3
	Remove damaged props.

	Fire
	Keep electrical equipment ventilated. No smoking or naked flames.
	1
	5
	5
	Fire extinguisher available.

	Lighting
	Position lights to avoid glare or contact with users.
	1
	3
	3
	Adjust setup if required.

	Privacy
	Images handled in accordance with data protection requirements.
	1
	4
	4
	Inform users of photo use.

	Children
	Children supervised by a responsible adult.
	1
	4
	4
	Operator monitoring.

	Weather
	Outdoor setups suspended during unsafe weather.
	1
	4
	4
	Monitor conditions.

	Unauthorised access
	Restrict access to operating equipment.
	1
	3
	3
	Barrier/signage.

	Printer burns
	Avoid contact with hot printer components during operation.
	1
	2
	2
	Staff only access.

	Emergency
	Isolate power if safe, administer first aid and contact emergency services if required.
	0
	0
	N/A
	First aid available.



