Risk Assessment – Mechanical Rodeo Ride (Public Hire)
Persons Involved: Site Team / Trained Operators
Also Present: Members of the Public, Venue Staff
Equipment: Mechanical rodeo ride, inflatable safety bed, control console, RCD, barriers
Location: Various Public Event Locations

	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Manual handling
	Team lifts; handling aids.
	1
	3
	3
	Training.

	Installation
	Ride erected by trained staff to manufacturer instructions.
	1
	5
	5
	Pre-opening inspection.

	Anchorage/Stability
	Ride level and secured.
	1
	5
	5
	Monitor during event.

	Falls from ride
	Inflatable bed; controlled speed; E-stop.
	2
	4
	8
	Operator supervision.

	Unsuitable riders
	Age/height/weight & medical restrictions enforced.
	2
	4
	8
	Clear signage.

	Loose items
	Remove phones, keys, glasses.
	1
	3
	3
	Operator checks.

	Crowding
	Barriered queue.
	2
	2
	4
	Queue management.

	Electrical
	PAT, RCD, protected cables.
	1
	5
	5
	Daily checks.

	Weather
	Suspend in severe weather.
	1
	5
	5
	Weather monitoring.

	Emergency
	Emergency stop, first aid, call 999 if needed.
	1
	5
	5
	Incident records.



