Risk Assessment – Roller Slide Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of roller slide equipment for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of slide and equipment
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure components during transport and setup.
	Low

	Participant falling from slide
	Participants
	High
	Inspect slide and access arrangements; provide clear instructions; allow only one user at a time where required; supervise the activity.
	Low

	Collision at slide exit
	Participants/Spectators
	High
	Define the landing/exit zone; keep the area clear; ensure users leave promptly before the next participant proceeds.
	Low

	Incorrect use / climbing or unsafe descent
	Participants
	High
	Provide a safety briefing; prohibit climbing on the slide, standing, overtaking or unsafe behaviour; supervise continuously.
	Low

	Slips, trips and falls
	All
	Medium
	Operate on a clean, dry and level surface; keep access and exit areas clear; remove hazards promptly.
	Low

	Slide movement / instability
	Participants/Spectators
	High
	Position securely on a suitable surface; secure or stabilise as required; inspect before use and stop play if movement occurs.
	Low

	Damaged slide / equipment
	All
	High
	Inspect structure, surface, seams, steps and landing area before use; remove damaged equipment from service.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Provide appropriate age, size and ability restrictions and supervision; follow manufacturer's requirements.
	Low

	Overcrowding at access / exit
	Participants/Spectators
	Medium
	Control queues and numbers; maintain clear access and landing zones.
	Low

	Emergency access obstructed
	All
	Medium
	Position the slide so emergency routes, exits and venue access remain clear.
	Low

	Poor lighting / visibility
	Participants/Staff
	Medium
	Provide adequate lighting for the slide, access, landing and surrounding area.
	Low


Operational Controls
Set up the Roller Slide activity on suitable ground/surface with adequate clearance and access.
Inspect equipment before each use and provide a clear safety briefing before participation.
Control participant numbers and maintain clearly defined playing, access and spectator areas.
Prohibit running, pushing, climbing, deliberate misuse and other unsafe behaviour.
Follow manufacturer operating, participant, anchoring and weather requirements where applicable.
Stop the activity immediately if equipment is damaged, unstable or conditions become unsafe.
Emergency Procedures
Stop the Roller Slide activity immediately following any incident or unsafe condition.
Ensure participants leave the active area safely and keep emergency routes clear.
Provide first aid where required and contact emergency services if necessary.
Remove damaged equipment from service and record all accidents and near misses.
Inspection Checklist
Equipment structure and components stable, secure and free from damage.
Playing/activity surface clean and free from defects or trip hazards.
Access, exit and spectator exclusion areas clearly defined.
Emergency routes and venue access remain clear.
Participant capacity, supervision and restrictions clearly established.
Training Requirements
Staff trained in safe Roller Slide operation, equipment inspection, participant briefing, supervision, crowd/access control, emergency procedures and incident response.
