Risk Assessment – Scalextric Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of an indoor archery stall using low-poundage bows and suction-cup or foam safety arrows for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; keep components secure during transport and setup.
	Low

	Participant struck by or hit by a car
	Participants/Spectators
	Medium
	Keep the track within a controlled play area; prohibit throwing cars or equipment; supervise operation.
	Low

	Finger trapping at track joints or moving components
	Participants
	Medium
	Give clear instructions; keep fingers clear of moving parts and track connections; supervise younger users.
	Low

	Electrical equipment / cable hazard
	Participants/Staff
	Medium
	Inspect power supplies, controllers and cables before use; route cables away from walkways; isolate defective equipment.
	Low

	Trips around track and cables
	All
	Medium
	Keep the surrounding floor clear; secure or route cables away from pedestrian routes; maintain good housekeeping.
	Low

	Damaged track, cars or controllers
	All
	Medium
	Inspect all components before each session and remove damaged items from use.
	Low

	Track sections becoming displaced
	Participants
	Medium
	Set up on a stable, level surface; check track connections before use and during operation.
	Low

	Incorrect use of controllers
	Participants
	Medium
	Provide a clear demonstration and safety briefing; supervise use; stop unsafe operation.
	Low

	Overcrowding around the racing table
	Participants/Spectators
	Medium
	Control participant numbers; maintain adequate space around the equipment; supervise queues and spectators.
	Low

	Spectators interfering with track
	Public
	Medium
	Define the play area and prevent spectators from reaching across or interfering with the track during racing.
	Low

	Small parts / cars presenting choking hazard
	Young children/Participants
	High
	Follow manufacturer age guidance; keep small components controlled; supervise younger participants closely.
	Low

	Slips or falls
	All
	Medium
	Operate on a clean, level and suitable surface; keep loose equipment and packaging away from walkways.
	Low

	Participant behaviour / disputes during racing
	Participants
	Medium
	Set clear rules before play; prohibit pushing or unsafe behaviour; staff supervise and intervene when necessary.
	Low

	Inadequate lighting / visibility
	Participants/Staff
	Medium
	Provide adequate lighting so track, controls, cables and surrounding hazards are clearly visible.
	Low


Operational Controls
 Set up on a suitable, level surface with adequate space around the Scalextric track.
 Give participants a clear safety briefing covering controllers, track use and safe handling of cars and components.
 Keep loose components controlled and prevent participants from reaching across or interfering with the track while racing.
 Maintain appropriate supervision, particularly where children are participating.
 Stop activity immediately if unsafe behaviour, electrical faults, damaged equipment or unsafe conditions occur.
Emergency Procedures
 Stop the Scalextric system immediately following any incident.
 Provide first aid where required and contact emergency services if necessary.
 Isolate damaged or defective electrical equipment and prevent further use.
 Record all accidents and near misses.
Inspection Checklist
 Track sections and connectors free from damage.
 Cars free from damage and suitable for use.
 Controllers and power supply free from visible damage.
 Cables and plugs free from visible damage and routed safely.
 Track stable and securely positioned.
Training Requirements
 Staff trained in safe Scalextric operation, manual handling, customer briefing, supervision, emergency procedures and equipment inspection.






