Risk Assessment – Tea Cups Ride Hire (HSE/AAIAC Style)
Activity Description
Delivery, installation, operation, supervision and dismantling of a Tea Cups Ride for temporary hire at events. The ride must only be operated by trained personnel in accordance with the manufacturer's instructions.
Persons at Risk
Operators, participants, staff, spectators, contractors and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup and dismantling
	Staff
	Medium
	Use safe lifting techniques and mechanical aids where required.
	Low

	Entrapment or pinch points
	Participants/Operators
	High
	Guard moving parts, conduct pre-use inspections and supervise continuously.
	Low

	Falls while boarding or exiting
	Participants
	High
	Only board/unload when ride is stationary; assist children where required.
	Low

	Dizziness or nausea from spinning
	Participants
	Medium
	Display health restrictions and stop participation if riders become unwell.
	Low

	Mechanical or electrical failure
	All
	High
	Daily inspections, planned maintenance and emergency stop testing before operation.
	Low

	Trips around ride perimeter
	All
	Medium
	Maintain clear walkways, barriers and secure cables.
	Low

	Unauthorised access
	Public
	Medium
	Use barriers and controlled access points.
	Low

	Adverse weather (outdoor use)
	All
	High
	Suspend operation during high winds or unsafe weather conditions.
	Low


Operational Controls
Install on a firm, level surface.
Operate only by trained personnel.
Carry out daily pre-use inspections.
Enforce rider height, age and health restrictions.
Maintain barriers throughout operation.
Do not exceed manufacturer passenger limits.
Emergency Procedures
Use the emergency stop immediately if required.
Evacuate passengers safely following manufacturer guidance.
Provide first aid and contact emergency services if necessary.
Isolate defective equipment and record all incidents.
Inspection Checklist
Ride securely assembled.
Emergency stop tested.
Safety gates and restraints functioning correctly.
Electrical connections secure.
Ride area clean and barriers correctly positioned.
Training Requirements
Operators trained in ride operation, passenger management, emergency procedures, inspections and manual handling.
