Risk Assessment – Trampoline Hire Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of trampoline hire equipment for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of trampoline and equipment
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure components during transport and setup.
	Low

	Trampoline instability / movement
	Participants
	High
	Set up on suitable firm, level ground; assemble correctly; secure and stabilise as specified; inspect before use.
	Low

	Participant falling / jumping injury
	Participants
	High
	Follow manufacturer capacity and operating rules; supervise use; control numbers; prohibit unsafe jumping, flips or rough play unless specifically permitted.
	Low

	Collision between participants
	Participants
	High
	Limit occupancy to the manufacturer's safe capacity; allow only suitable users together; supervise continuously.
	Low

	Falls from trampoline / access area
	Participants
	High
	Provide safe access and exit; keep surrounding area clear; prevent climbing onto or off the trampoline from unsafe locations.
	Low

	Damaged mat, springs, frame or padding
	Participants/Staff
	High
	Inspect mat, frame, springs, padding, enclosure and fixings before each use; remove defective equipment from service.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Apply manufacturer age, size and ability restrictions; provide suitable supervision.
	Low

	Trips around trampoline
	All
	Medium
	Maintain clear, level and dry surrounding area; keep bags and equipment away from access points.
	Low

	Weather conditions
	All
	High
	For outdoor use, follow manufacturer's weather and wind requirements; stop operation in unsuitable conditions.
	Low

	Overcrowding / spectator access
	Participants/Spectators
	Medium
	Control queues and numbers; keep spectators outside the active area unless authorised.
	Low

	Emergency access obstructed
	All
	Medium
	Position the trampoline so emergency routes, exits and venue access remain clear.
	Low


Operational Controls
Set up the Trampoline Hire activity on suitable ground/surface with adequate clearance and access.
Inspect equipment before each use and provide a clear safety briefing before participation.
Control participant numbers and maintain clearly defined playing, access and spectator areas.
Prohibit running, pushing, climbing, deliberate misuse and other unsafe behaviour.
Follow manufacturer operating, participant and site requirements where applicable.
Stop the activity immediately if equipment is damaged, unstable or conditions become unsafe.
Emergency Procedures
Stop the Trampoline Hire activity immediately following any incident or unsafe condition.
Ensure participants leave the active area safely and keep emergency routes clear.
Provide first aid where required and contact emergency services if necessary.
Remove damaged equipment from service and record all accidents and near misses.
Inspection Checklist
Equipment structure and components stable, secure and free from damage.
Activity surface and surrounding area clean and free from defects or trip hazards.
Access, exit and spectator areas clearly defined.
Emergency routes and venue access remain clear.
Participant capacity, supervision and restrictions clearly established.
Training Requirements
Staff trained in safe Trampoline Hire operation, equipment inspection, participant briefing, supervision, crowd/access control, emergency procedures and incident response.
