Risk Assessment – Arcade Machines Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, operation and collection of arcade machines for temporary hire at events.
Persons at Risk
Staff, hirers, participants, children and spectators.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of heavy machines
	Staff
	High
	Use suitable lifting equipment and team lifts; trained staff only.
	Low

	Machine instability or tipping
	All
	Medium
	Position on firm, level ground and check stability before use.
	Low

	Electrical hazards
	All
	Medium
	PAT-tested equipment, visual inspection, RCD protection and undamaged cables.
	Low

	Trips from trailing cables
	All
	Medium
	Route and secure cables using cable covers where necessary.
	Low

	Misuse or rough play
	Participants
	Medium
	Provide operating instructions and supervise younger users.
	Low

	Equipment damage or malfunction
	All
	Medium
	Inspect before dispatch and after collection; remove defective equipment from service.
	Low


Operational Controls
Inspect machine, plug and cable before each hire.
Set up on a firm, level surface with adequate ventilation.
Keep food and drinks away from electrical equipment.
Do not move the machine while powered.
Disconnect power before maintenance or inspection.
Emergency Procedures
Switch off and isolate power if a fault develops.
Stop use immediately if equipment becomes unstable or damaged.
Provide first aid if required and report all incidents.
Inspection Checklist
Cabinet undamaged.
Power cable and plug in good condition.
Controls functioning correctly.
Machine stable.
No exposed electrical components.
Training Requirements
Staff trained in manual handling, electrical safety, setup, inspection and customer briefing.
