Risk Assessment – Baby Rodeo Ride (Public Hire)
Persons Involved: Site Team / Trained Operators
Also Present: Children, Parents/Guardians, Venue Staff
Equipment: Children's mechanical rodeo ride, inflatable safety surround, control unit, RCD, barriers
Location: Various Public Event Locations

	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Manual handling
	Team lifting and safe handling.
	1
	3
	3
	Training.

	Installation
	Installed by trained staff.
	1
	5
	5
	Pre-use inspection.

	Falls
	Inflatable surround; slow ride settings.
	1
	4
	4
	Continuous supervision.

	Unsuitable riders
	Age/height/weight limits enforced.
	2
	3
	6
	Parent advised.

	Parent interference
	Parents remain outside barrier during operation.
	2
	2
	4
	Operator instruction.

	Loose items
	Remove glasses and loose objects.
	1
	2
	2
	Checks before ride.

	Electrical
	PAT tested with RCD.
	1
	5
	5
	Daily inspection.

	Crowd management
	Barriered queue.
	2
	2
	4
	Staff supervision.

	Weather
	Suspend outdoors in severe weather.
	1
	5
	5
	Monitor conditions.

	Emergency
	Use E-stop; first aid; call 999 if required.
	1
	5
	5
	Incident reporting.



