Risk Assessment – Batak Pro Hire (HSE/AAIAC Style)
Activity Description
Assessment for transport, setup, operation, supervision and dismantling of the Batak Pro electronic reaction training system.
Persons at Risk
Participants, operators, staff, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Use two-person lift/trolley
	Low

	Electrical hazards
	All
	High
	PAT tested equipment and RCD
	Low

	Trailing cables
	All
	Medium
	Secure cables with covers
	Low

	Equipment instability
	All
	Medium
	Level setup and pre-use inspection
	Low

	Participant collision
	Participants
	Medium
	One user at a time; clear operating area
	Low

	Overexertion
	Participants
	Medium
	Allow rest breaks; stop if unwell
	Low

	Slips and trips
	All
	Medium
	Keep area clear and dry
	Low

	Unauthorised use
	Public
	Medium
	Operator supervision
	Low

	Fire risk
	All
	Medium
	Keep exits clear; isolate power if required
	Low

	Dismantling
	Staff
	Medium
	Power off before dismantling; safe manual handling
	Low


Operational Controls
Inspect frame, target pads, electronics, cables, power supply and signage before use. Supervise participants throughout.
Emergency Procedures
Switch off power, isolate equipment, provide first aid if required and remove defective equipment from service.
Inspection Checklist
Frame, targets, control unit, power cable, RCD, fixings, signage and surrounding floor area.
Training Requirements
Manual handling, setup, electrical safety, operation, supervision and emergency procedures.
