Risk Assessment – Inflatable Combi Sports Arena Hire
Activity: Inflatable Combi Sports Arena Hire

Activity Description
This assessment covers the delivery, installation, operation, supervision and dismantling of an inflatable Combi Sports Arena for multi-sport activities. It aligns with UK H&S legislation, PUWER, BS EN 14960 and HSE guidance.
Persons at Risk
Participants, children, adults, operators, installation staff, spectators, organisers and members of the public.
Risk Assessment
See key hazards and controls below.
	Hazard
	Persons
	Initial
	Controls
	Residual

	Manual handling
	Staff
	Medium
	Team lifting and trolleys; trained staff
	Low

	Uneven ground
	Users
	High
	Install only on level inspected ground
	Low

	Anchor failure
	Users
	High
	Secure all anchors/ballast to BS EN14960
	Low

	High winds
	Everyone
	High
	Monitor wind; close above manufacturer/24mph limit
	Low

	Electrical hazards
	Everyone
	High
	PAT tested blower, RCD, protected cables
	Low

	Collisions
	Users
	High
	Supervision and safe play rules
	Medium

	Overcrowding
	Users
	High
	Limit capacity and separate ages
	Low

	Equipment damage
	Everyone
	High
	Pre-use inspections
	Low

	Fire
	Everyone
	High
	No smoking; emergency plan
	Low


Emergency Procedures
Evacuate on blower failure, high winds, fire or medical emergency. Disconnect power when safe and contact emergency services if required.
