Risk Assessment – Inflatable Gladiators Hire (HSE/AAIAC Style)
Activity Description
This assessment covers the transport, installation, inflation, operation, supervision and dismantling of an inflatable gladiators game used at events.
Persons at Risk
Participants, ball throwers, children, adults, operators, installation staff, spectators and members of the public.
Detailed Risk Assessment
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Team lifting and handling aids.
	Low

	Inflation/electrical blower
	Staff/Public
	High
	PAT tested blower, RCD protection, cables protected.
	Low

	Poor anchoring
	Everyone
	High
	Anchor to manufacturer specification.
	Low

	Falls from podiums
	Participants
	High
	Safety briefing, one pair at a time.
	Low

	Collision with opponent
	Participants
	Medium
	Padded pugil sticks, matched by age/size.
	Low

	High winds
	Everyone
	High
	Cease use if wind exceeds manufacturer limits.
	Low

	Trips
	Everyone
	Medium
	Keep perimeter and cables clear.
	Low

	Spectator encroachment
	Public
	Medium
	Barrier around activity and operator control.
	Low

	Equipment failure
	Everyone
	High
	Daily inspection before use.
	Low

	Dismantling hazards
	Staff
	Medium
	Controlled deflation and safe manual handling.
	Low


Operational Controls
Inspect the tank, frame, release mechanism, water level, throwing target, barriers and signage before opening.
Emergency Procedures
Stop activity, assist participant from the tank, administer first aid if required, isolate faulty equipment and follow site evacuation procedures.
Inspection Checklist
Tank, frame, seat, release mechanism, target, water quality, drain valve, hoses, barriers and signage.
Training Requirements
Manual handling, safe setup, water safety awareness, emergency procedures, first aid awareness and daily inspections.
