Risk Assessment – Laser Tag Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of a laser tag arena using infrared taggers, sensor vests/headbands and inflatable or portable obstacles for temporary hire at events.
Persons at Risk
Installation staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of equipment
	Staff
	Medium
	Use safe lifting techniques and team lifts where required.
	Low

	Trips over obstacles, cables or arena features
	Participants
	High
	Maintain clear walkways, secure cables, space obstacles appropriately and brief players before play.
	Low

	Collisions between participants
	Participants
	Medium
	Limit player numbers, prohibit running into obstacles, enforce game rules and provide supervision.
	Low

	Slips on uneven or wet surfaces
	All
	Medium
	Use only on suitable level surfaces and suspend play if conditions become unsafe.
	Low

	Electrical hazards from powered equipment
	All
	Medium
	PAT-tested equipment, inspect cables before use and use RCD protection.
	Low

	Equipment malfunction
	Participants
	Medium
	Inspect taggers, sensors and bases before use; remove faulty equipment from service.
	Low

	Spectators entering play area
	Public
	Medium
	Create a clearly defined exclusion zone and supervise continuously.
	Low

	Damaged arena equipment
	All
	Medium
	Inspect before each hire and quarantine damaged equipment.
	Low


Operational Controls
Set up on a level surface with adequate space around the arena.
Provide a full safety briefing before each game.
Enforce no physical contact, climbing or aggressive behaviour.
Ensure continuous adult supervision throughout operation.
Stop play immediately if unsafe conditions arise.
Emergency Procedures
Cease the game immediately following an accident or equipment failure.
Isolate faulty electrical equipment.
Provide first aid and contact emergency services where necessary.
Record incidents and remove defective equipment from service.
Inspection Checklist
Laser taggers and sensors functioning correctly.
Inflatable or portable obstacles secure and undamaged.
Power supplies, chargers and cables in good condition.
RCD tested and operational where applicable.
Arena free from hazards before opening.
Training Requirements
Staff trained in manual handling, electrical safety, safe arena setup, equipment operation, emergency procedures and customer safety briefings.
