Risk Assessment – Last Man Standing Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, operation, supervision and dismantling of an inflatable Last Man Standing attraction.
Persons at Risk
Participants, operators, spectators, staff and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Team lifting and handling aids
	Low

	Incorrect anchoring
	Everyone
	High
	Anchor to manufacturer specification
	Low

	Electrical hazards
	Everyone
	High
	PAT tested equipment with RCD
	Low

	Trips from cables
	Everyone
	Medium
	Use cable covers and secure routing
	Low

	Rotating boom impact
	Participants
	High
	Operator-controlled speed and safety briefing
	Low

	Falls from podium
	Participants
	High
	Inflatable landing surface and supervision
	Low

	Participant collision
	Participants
	Medium
	Limit player numbers and supervise
	Low

	High winds
	Everyone
	High
	Do not operate in unsuitable weather
	Low

	Unauthorised access
	Public
	Medium
	Barrier off attraction
	Low

	Dismantling
	Staff
	Medium
	Power off, deflate safely and use correct lifting
	Low


Operational Controls
Inspect inflatable, rotating boom, controls, anchors, blower, mats and barriers before use. Continuous operator supervision required.
Emergency Procedures
Stop the attraction immediately, isolate power, assist injured participants, administer first aid and remove defective equipment from service.
Inspection Checklist
Inflatable, seams, rotating arm, motor, control unit, blower, RCD, anchors, mats, barriers and signage.
Training Requirements
Manual handling, inflatable setup, electrical safety, operation of rotating controls, emergency procedures and daily inspections.
