Risk Assessment – Magic Mirror Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, operation, supervision and dismantling of an interactive Magic Mirror photo system.
Persons at Risk
Participants, operators, staff, venue personnel and the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Two-person lift/use trolley
	Low

	Electrical equipment
	All
	High
	PAT tested equipment, RCD protection
	Low

	Trailing cables
	All
	Medium
	Cable covers and tidy routing
	Low

	Mirror/frame instability
	All
	High
	Secure setup and pre-use inspection
	Low

	Glass/acrylic damage
	Participants
	Medium
	Inspect before use; remove damaged unit
	Low

	Trips and slips
	All
	Medium
	Keep surrounding area clear and dry
	Low

	Crowding
	Public
	Medium
	Manage queues and supervise
	Low

	Equipment misuse
	Participants
	Medium
	Operator assistance and supervision
	Low

	Fire
	All
	Medium
	Keep exits clear and isolate power if required
	Low

	Dismantling
	Staff
	Medium
	Power off and use safe manual handling
	Low


Operational Controls
Inspect mirror, frame, camera, printer, lighting, cables and accessories before use. Continuous supervision recommended.
Emergency Procedures
Switch off power, isolate electrical supply, administer first aid if required and remove defective equipment from service.
Inspection Checklist
Mirror, frame, camera, printer, touch screen, lighting, cables, RCD, props and surrounding area.
Training Requirements
Manual handling, setup, electrical safety, customer supervision and emergency procedures.
