Risk Assessment – Penalty Shootout Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, inflation, operation, supervision and dismantling of an inflatable penalty shootout game.
Persons at Risk
Participants, operators, spectators, staff and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Team lifting/manual handling aids
	Low

	Incorrect anchoring
	Everyone
	High
	Secure to manufacturer specification
	Low

	Electrical blower
	Everyone
	High
	PAT tested with RCD protection
	Low

	Trips from cables
	Everyone
	Medium
	Cable covers and tidy routing
	Low

	Ball striking spectators
	Public
	Medium
	Barrier off shooting area
	Low

	Player collision
	Participants
	Medium
	One player shoots at a time
	Low

	Slips and trips
	Everyone
	Medium
	Keep area clear and dry
	Low

	High winds
	Everyone
	High
	Do not operate in unsafe weather
	Low

	Unauthorised access
	Public
	Medium
	Operator supervision
	Low

	Dismantling
	Staff
	Medium
	Power off, deflate safely and team lift
	Low


Operational Controls
Inspect inflatable, seams, anchors, blower, balls, barriers and signage before use. Continuous supervision required.
Emergency Procedures
Stop activity, isolate power, provide first aid if necessary and remove faulty equipment from service.
Inspection Checklist
Inflatable, seams, anchors, blower, RCD, footballs, barriers, mats and signage.
Training Requirements
Manual handling, inflatable setup, electrical safety, supervision, emergency procedures and inspections.
