Risk Assessment – Photo Booth Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, operation, supervision and dismantling of a portable photo booth for events.
Persons at Risk
Participants, operators, staff, venue personnel and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Two-person lift/use trolley
	Low

	Electrical equipment
	Everyone
	High
	PAT tested equipment with RCD protection
	Low

	Trailing cables
	Everyone
	Medium
	Secure with cable covers
	Low

	Booth instability
	Everyone
	High
	Assemble to manufacturer instructions and inspect
	Low

	Trips and slips
	Everyone
	Medium
	Keep area tidy and dry
	Low

	Crowding/queuing
	Public
	Medium
	Manage queues and maintain clear walkways
	Low

	Equipment damage
	Everyone
	Medium
	Operator supervision; restrict access to equipment
	Low

	Fire risk
	Everyone
	Medium
	Keep away from heat sources; maintain clear exits
	Low

	Unauthorised use
	Public
	Medium
	Supervise throughout hire
	Low

	Dismantling
	Staff
	Medium
	Power off before dismantling; use safe manual handling
	Low


Operational Controls
Inspect booth structure, camera, printer, lighting, cables and accessories before use. Ensure continuous supervision where appropriate.
Emergency Procedures
Switch off and isolate electrical supply, provide first aid if required, and remove faulty equipment from service.
Inspection Checklist
Booth frame, camera, printer, lighting, cables, RCD, props, signage and surrounding floor area.
Training Requirements
Manual handling, setup, electrical safety, customer supervision and emergency procedures.
