Risk Assessment – Princess Bouncy Castle Hire (HSE/AAIAC Style)
Activity Description
Delivery, installation, supervision guidance, use and dismantling of a princess-themed inflatable bouncy castle for temporary hire at events.
Persons at Risk
Installation staff, hirers, supervisors, children, parents/carers and spectators.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use correct lifting techniques and team lifts where required.
	Low

	Inflatable movement due to wind
	Users/Public
	High
	Install on suitable surface, anchor in accordance with manufacturer instructions, do not operate in unsafe weather.
	Low

	Trips over blower or cables
	All
	Medium
	Secure blower, protect and route cables away from walkways using RCD-protected supply.
	Low

	Falls from inflatable
	Children
	Medium
	No climbing on walls; enforce user height/age limits; adult supervision at all times.
	Low

	Collisions between users
	Children
	Medium
	Separate users by size where possible and limit numbers to manufacturer guidance.
	Low

	Failure of blower or power supply
	Users
	Medium
	Stop use immediately, evacuate safely and inspect equipment before reuse.
	Low

	Entrapment at entrance or walls
	Children
	Medium
	Keep entrance clear and prohibit rough play, flips and wrestling.
	Low

	Damaged inflatable
	All
	Medium
	Inspect before each hire and remove from service if damaged.
	Low


Operational Controls
Install on level ground with required safety mats.
Anchor using stakes or ballast as appropriate.
Brief hirer on safe operation and weather limits.
Constant responsible adult supervision during use.
Cease operation immediately during high winds, heavy rain or electrical storms.
Emergency Procedures
Stop use and evacuate immediately if blower fails or inflatable becomes unstable.
Isolate electrical supply if a fault occurs.
Administer first aid and contact emergency services if required.
Report all incidents and quarantine damaged equipment.
Inspection Checklist
Inflatable fabric free from tears.
Anchor points secure.
Blower operating correctly.
Power cable and RCD in good condition.
Safety mats correctly positioned.
Training Requirements
Staff trained in safe inflatable installation, anchoring, weather assessment, manual handling, electrical safety and customer safety briefing.
