Risk Assessment – Rodeo Bull Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, operation, supervision and dismantling of a mechanical rodeo bull with inflatable safety bed.
Persons at Risk
Participants, operators, spectators, staff and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Team lift/use handling aids
	Low

	Electrical supply
	All
	High
	PAT tested equipment and RCD
	Low

	Incorrect setup
	All
	High
	Trained operator and pre-use checks
	Low

	Falls from bull
	Participants
	High
	Inflatable landing bed and controlled speed
	Low

	Impact with bull
	Participants
	High
	Operator supervision and emergency stop
	Low

	Entrapment
	Participants
	Medium
	Clear operating zone and inspections
	Low

	Trips from cables
	All
	Medium
	Secure cable routing
	Low

	Unauthorised access
	Public
	Medium
	Barriers and controlled entry
	Low

	High winds (outdoors)
	All
	High
	Do not operate in adverse weather
	Low

	Dismantling
	Staff
	Medium
	Power off and safe manual handling
	Low


Operational Controls
Inspect bull, inflatable bed, controls, emergency stop, blower, anchors and barriers before use. Operator present at all times.
Emergency Procedures
Stop ride immediately using emergency stop, isolate power, provide first aid and remove defective equipment from service.
Inspection Checklist
Bull mechanism, inflatable bed, blower, RCD, emergency stop, anchors, mats, barriers and signage.
Training Requirements
Manual handling, setup, electrical safety, ride operation, emergency procedures and daily inspections.
