Risk Assessment – High Striker Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, operation and collection of a High Striker strength tester for temporary hire at events.
Persons at Risk
Staff, hirers, participants, spectators and children.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during transport/setup
	Staff
	High
	Use team lifts or mechanical aids; trained staff only.
	Low

	Toppling or instability
	All
	High
	Assemble on firm, level ground and secure all components before use.
	Low

	Impact from swinging mallet
	Participants/Spectators
	High
	Create an exclusion zone around the striker; only one player at a time.
	Low

	Flying mallet if grip lost
	All
	Medium
	Inspect mallet before use and ensure users maintain a secure grip.
	Low

	Finger/hand injuries
	Participants
	Medium
	Keep hands clear of the striking area and provide clear instructions.
	Low

	Trips around equipment
	All
	Medium
	Keep the surrounding area free from obstacles and loose equipment.
	Low

	Damaged equipment
	All
	Medium
	Inspect before dispatch, during setup and after collection; remove damaged items from service.
	Low


Operational Controls
Set up on firm, level ground.
Inspect tower, bell mechanism, base and mallet before use.
Only one participant permitted in the striking area at a time.
Maintain a clear exclusion zone around the attraction.
Remove equipment from use if damaged or unstable.
Emergency Procedures
Stop use immediately if any component becomes loose or unstable.
Provide first aid where required.
Report and record all incidents and equipment defects.
Inspection Checklist
Base secure.
Tower vertical and stable.
Bell mechanism functioning.
Mallet in good condition.
Area free from trip hazards.
Training Requirements
Staff trained in manual handling, safe assembly, inspection, customer briefing and supervision.
