Risk Assessment – Surf Simulator Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, operation, supervision and dismantling of a mechanical surf simulator with inflatable safety bed.
Persons at Risk
Participants, operators, spectators, staff and the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Team lifting/use handling aids
	Low

	Electrical equipment
	All
	High
	PAT tested, RCD protected
	Low

	Incorrect setup
	All
	High
	Trained staff and pre-use checks
	Low

	Falls from simulator
	Participants
	High
	Inflatable landing bed, controlled operation
	Low

	Impact with moving surfboard
	Participants
	High
	Operator supervision and emergency stop
	Low

	Entrapment
	Participants
	Medium
	Routine inspections and clear operating zone
	Low

	Trips from cables
	All
	Medium
	Secure cable routing and covers
	Low

	Unauthorised access
	Public
	Medium
	Barriers and supervised entry
	Low

	Adverse weather (outdoors)
	All
	High
	Do not operate in unsafe weather
	Low

	Dismantling
	Staff
	Medium
	Power off, deflate safely and manual handling controls
	Low


Operational Controls
Inspect simulator, inflatable bed, emergency stop, controls, blower, anchors, mats and barriers before operation. Continuous trained supervision is required.
Emergency Procedures
Stop the simulator immediately, isolate electrical supply, administer first aid if required and remove defective equipment from service.
Inspection Checklist
Mechanical surf unit, inflatable bed, blower, RCD, emergency stop, anchors, mats, barriers and safety signage.
Training Requirements
Manual handling, safe setup, electrical safety, simulator operation, emergency procedures and daily inspections.
