RISK ASSESSMENT



Funday Entertainment Limited

|  |  |  |  |
| --- | --- | --- | --- |
| **LOCATION:** | Various Locations |  |   |
| **OPERATION/PROCESS:** | Safe installation and operation of dunk tank |
| **HAZARDS IDENTIFIED:** | 1. Being struck by moving equipment
2. Drowning ,
3. Slips/ Trips & falls,
4. Minor injuries
 |
| **SECONDARY HAZARDS:** | Other people,  |
| **EXPOSED PERSONS:** | Funday staff, participants, members of the public (i.e. other persons in the area) |
| **FREQUENCY OF EXPOSURE:** | Event dates | **DURATION OF EXPOSURE:** As per event hours |
| ***RISK = LIKELIHOOD X SEVERITY*** |
| ***LIKELIHOOD*****0** = Zero to very low**1** = Very unlikely**2** = Unlikely | **3** = Likely**4** = Very likely**5** = Almost certain | ***SEVERITY*****0** = No injury or illness**1** = First aid injury or illness**2** = Minor injury or illness | **3** = “ 3 day “ injury or illness**4** = Major injury or illness **5** = Fatality, disablement injury, etc |
| **Risk Values:** LOW = **1 to 8** MEDIUM = **9 to 16** HIGH = **17 to 25** |
| **Activity Risk Rating:** *Likelihood* ***4*** *X Severity* ***3*** *= Total* ***12*** |
| **Activity Risk Value*:*** *LOW* ***MEDIUM*** *HIGH* |
| **CONTROL MEASURES** **Steps to be taken to avoid an accident or incident leading to an injury:** | 1. There is a minimum height restriction of 4ft and age restriction of 8 years old.
2. The operator/ supervisor will provide assistance to those entering or exiting the tank to help prevent slips/ trips or falls on the steps.
3. The item must be cordoned off when not in use and access into the tank will be prevented.
4. Water will only remain in the tank while absolutely necessary.
5. A fully competent operator will be in attendance and watch the equipment at all times who is able to enter the water if necessary.
6. All tennis balls are to be thrown at targets only.
7. The client must take all necessary precautions to prevent the hose becoming a trip and fall hazard whilst the dunk is being filled up.
8. No shoes or boots to be worn.
9. All sharp and electrical objects to be removed.
10. To be setup away from power cabling.
 |
|  |  |
| **Residual Risk Rating*:*** *Likelihood* ***2***  *X Severity* ***3***  *= Total* ***6*** |
| **MONITORING RESULTS:** | The Funday Manager is to ensure the above is adhered to then the risk is acceptable. |
| **REVIEW DATE:** | At regular intervals, not to exceed 12 months or when circumstances change. |
| **RESIDUAL RISK RATING: LOW** |
| **ASSESSOR:** | Andre Rayson | **POSITION:** | Senior Health & Safety Advisor |