Risk Assessment – Air Hockey Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, use and collection of an air hockey table for events.
Persons at Risk
Staff, hirers, participants, spectators.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	Medium
	Use safe lifting techniques and two-person lifts.
	Low

	Trips
	All
	Medium
	Keep surrounding area clear.
	Low

	Electrical faults
	All
	Medium
	PAT tested, inspect cables, use RCD.
	Low

	Finger impact
	Players
	Low
	Supervise children and prevent rough play.
	Low

	Equipment damage
	All
	Low
	Inspect before and after hire.
	Low


Operational Controls
Inspect before dispatch.
Provide user instructions.
Do not use if damaged.
Emergency Procedures
Stop use if unsafe.
Disconnect power before inspection.
Report incidents.
Inspection Checklist
Surface intact.
Cables undamaged.
Unit clean.
Feet stable.
Training Requirements
Manual handling, setup, inspection and customer briefing.
