Risk Assessment – Cash Grabber Hire
Activity: Hire and supervised operation of a Cash Grabber machine.
Equipment: Cash Grabber booth, blower, power supply, paper vouchers/tokens.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Back strain/crush injuries
	Two-person lift where required; use trolley
	Low

	Electrical equipment
	Staff, Users
	Electric shock
	PAT-tested equipment, RCD protection, visual inspection before use
	Low

	Trailing cables
	Public
	Trips and falls
	Use cable covers and route cables away from walkways
	Low

	Blower operation
	Users
	Minor injury from moving air
	Guarded blower, secure connections, supervise use
	Low

	Entrapment in booth
	Users
	Panic/minor injury
	Door opened immediately if required; operator present
	Low

	Slips when exiting
	Users
	Falls
	Keep floor dry and clear
	Low

	Horseplay
	Users
	Minor injuries
	Supervision and clear rules
	Medium

	Overcrowding
	Public
	Collisions
	One participant at a time
	Low

	Damaged equipment
	Users
	Cuts/equipment failure
	Inspect before every hire and remove defective equipment
	Low

	Fire exits obstructed
	Public
	Delayed evacuation
	Position away from emergency exits
	Low


Additional Control Measures
Operator or responsible adult to supervise at all times.
One participant inside the booth at any one time.
No food, drink or sharp objects inside the booth.
Inspect equipment before each hire.
Children to be supervised by an adult.
Emergency Procedures
Stop operation immediately if equipment becomes unsafe. Isolate electrical power if required, administer first aid, record all incidents, and remove defective equipment from service.
