Risk Assessment – Dance Machine Hire
Activity: Hire and supervised use of an electronic dance machine.
Equipment: Dance machine, dance platform, display screen, sound system, power supply, extension leads, RCD.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Back strains
	Two-person lift; trolley
	Low

	Electrical equipment
	Staff, Users
	Electric shock
	PAT tested, RCD, visual inspection
	Low

	Trailing cables
	Public
	Trips
	Cable covers
	Low

	Slips/falls
	Participants
	Sprains
	Clean, dry, level surface
	Medium

	Collisions
	Participants
	Minor injuries
	Adequate spacing
	Low

	Fatigue
	Participants
	Dizziness
	Breaks and hydration
	Low

	Horseplay
	Participants
	Injury
	Supervision
	Medium

	Damaged equipment
	Users
	Cuts/shock
	Inspect before hire
	Low

	Blocked fire exits
	Public
	Evacuation delay
	Keep exits clear
	Low

	High sound
	Users
	Hearing discomfort
	Safe volume
	Low


Additional Control Measures
Inspect before every hire.
Operate on a firm, level surface.
No food or drink near equipment.
Continuous supervision for children.
Keep spectators clear.
Emergency Procedures
Stop use if faulty. Isolate power if required, administer first aid, record incidents and remove defective equipment.
