Comprehensive Risk Assessment – Electric Go Kart Hire (Public Events)
Activity Details
Activity: Electric Go Kart Hire
Suitable for: Schools, Councils, Corporate Events, Public Events
Operators: Trained staff only
Review: Annually or after any incident
Comprehensive Hazard Assessment
	Hazard
	Control Measures
	L
	S
	Risk
	Further Action

	Transport & unloading
	Team lifting, ramps, PPE, exclusion zone.
	1
	3
	3
	Training

	Track construction
	Level surface, barriers secured, marshal gates.
	1
	5
	5
	Inspection

	Kart mechanical failure
	Daily inspection of steering, brakes, throttle, tyres, seat, emergency stop.
	1
	5
	5
	Maintenance log

	Battery hazards
	Manufacturer chargers only; ventilated charging area; damaged batteries quarantined.
	1
	5
	5
	Battery register

	Electrical safety
	PAT tested chargers, RCD protection, cable covers.
	1
	5
	5
	Daily checks

	Collision
	Speed governors, one-way system, marshals, briefing.
	2
	4
	8
	Continuous supervision

	Pedestrian intrusion
	Barriered circuit and controlled access.
	1
	5
	5
	Marshal

	Driver behaviour
	No bumping, racing or reckless driving.
	2
	3
	6
	Remove offenders

	Unsuitable participants
	Age/height/weight restrictions and medical screening.
	2
	4
	8
	Operator checks

	PPE
	Helmets fitted where required.
	1
	4
	4
	Inspect PPE

	Weather
	Suspend in heavy rain, lightning or unsafe conditions.
	1
	5
	5
	Weather monitoring

	Fire
	CO2/dry powder extinguisher near charging.
	1
	5
	5
	Emergency plan

	Emergency
	Emergency stop, isolate track, first aid, 999 if required.
	1
	5
	5
	Incident report


Daily Pre-Opening Checklist
Inspect all karts.
Check steering and brakes.
Test emergency stop.
Inspect barriers.
Check batteries.
Inspect chargers and cables.
Confirm first aid kit and fire extinguisher.
Complete inspection log.
Operator Responsibilities
Conduct safety briefing.
Enforce driver rules.
Monitor speed and behaviour.
Stop activity if unsafe.
Record incidents.
Emergency Action Plan
Stop all karts immediately.
Isolate power.
Provide first aid.
Call emergency services if required.
Secure scene.
Complete accident report.
Applicable Guidance
Health and Safety at Work etc. Act 1974
Management of Health and Safety at Work Regulations 1999
Provision and Use of Work Equipment Regulations (PUWER) 1998
Electricity at Work Regulations 1989
Manufacturer operating manual
