Risk Assessment – Inflatable Football Shooting Game (Public Hire)
Persons Involved: Site Team / Trained Operators
Also Present: Members of the Public, Venue Staff
Equipment: Inflatable football shooting game, blower, anchor stakes/sandbags, RCD, footballs
Location: Various Public Event Locations

	Hazard
	Existing Controls
	Likelihood
	Severity
	Risk
	Further Action

	Manual handling
	Safe lifting techniques and team lifts.
	1
	3
	3
	Training.

	Installation
	Installed to manufacturer instructions.
	1
	5
	5
	Pre-use inspection.

	Anchoring
	Secure with approved stakes/ballast.
	1
	5
	5
	Check regularly.

	Blower failure
	Stop use immediately if blower stops.
	1
	5
	5
	Inspect before restart.

	Inflation/Deflation
	No users during inflation or deflation.
	1
	5
	5
	Operator only.

	Wind & Weather
	Do not use above manufacturer wind limits (typically 24 mph/38 km/h); stop during heavy rain/thunderstorms.
	1
	5
	5
	Continuous monitoring.

	Trip hazards
	Secure cables; keep area tidy.
	1
	2
	2
	Routine checks.

	Ball strikes
	Only one shooter where required; netting fitted.
	2
	2
	4
	Supervision.

	Misuse
	No climbing or rough play.
	2
	3
	6
	Display rules.

	Electrical
	PAT-tested blower with RCD.
	1
	5
	5
	Daily inspection.

	HSE guidance
	Operate in line with HSE inflatable guidance and manufacturer manual.
	1
	4
	4
	Annual review.

	Emergency
	Stop use, provide first aid, call 999 if required.
	1
	5
	5
	Incident reporting.



