Risk Assessment – Inflatable Target Football Shootout Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of inflatable target football shootout equipment for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling of inflatable and equipment
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; secure equipment during transport and setup.
	Low

	Inflatable instability / inadequate anchoring
	Participants/Spectators
	High
	Set up on suitable firm, level ground; use specified anchoring; inspect before use and stop if movement occurs.
	Low

	Football striking participant / spectator
	Participants/Spectators
	High
	Define shooting and spectator zones; only one player shoots where appropriate; keep spectators clear.
	Low

	Ball leaving controlled area
	Participants/Spectators
	Medium
	Position and secure the inflatable appropriately; maintain clear boundaries; stop play if a ball leaves the controlled area.
	Low

	Incorrect kicking technique / misuse
	Participants
	Medium
	Provide instructions; prohibit kicking at people, excessive force, climbing and unsafe behaviour.
	Low

	Trips from footballs or equipment
	All
	Medium
	Keep unused balls in a designated area; collect displaced balls promptly; maintain clear walkways.
	Low

	Damaged inflatable / target
	All
	High
	Inspect inflatable, targets and footballs before each session; remove damaged equipment from service.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Provide clear instructions and appropriate supervision; consider participant ability and physical capability.
	Low

	Overcrowding
	Participants/Spectators
	Medium
	Control player numbers and queues; maintain clearly defined playing and spectator areas.
	Low

	Electrical equipment / blower
	Staff/Participants
	High
	Inspect blower, cables and connections; route cables safely and keep electrical connections dry.
	Low

	Emergency access obstructed
	All
	Medium
	Position the activity so emergency routes, exits and venue access remain clear.
	Low

	Poor lighting / visibility
	Participants/Staff
	Medium
	Provide adequate lighting so the target, ball, floor and surrounding hazards are clearly visible.
	Low


Operational Controls
Set up the Inflatable Target Football Shootout activity on suitable ground/surface with adequate clearance and access.
Inspect equipment before each use and provide a clear safety briefing before participation.
Control participant numbers and maintain clearly defined playing, access and spectator areas.
Prohibit running, pushing, climbing, deliberate misuse and other unsafe behaviour.
Follow manufacturer operating, participant, anchoring and weather requirements where applicable.
Stop the activity immediately if equipment is damaged, unstable or conditions become unsafe.
Emergency Procedures
Stop the Inflatable Target Football Shootout activity immediately following any incident or unsafe condition.
Ensure participants leave the active area safely and keep emergency routes clear.
Provide first aid where required and contact emergency services if necessary.
Remove damaged equipment from service and record all accidents and near misses.
Inspection Checklist
Equipment structure and components stable, secure and free from damage.
Activity surface clean and free from defects or trip hazards.
Access, exit and spectator areas clearly defined.
Emergency routes and venue access remain clear.
Participant capacity, supervision and restrictions clearly established.
Training Requirements
Staff trained in safe Inflatable Target Football Shootout operation, equipment inspection, participant briefing, supervision, crowd/access control, emergency procedures and incident response.
