Risk Assessment – Inflatable Volleyball Hire
Activity: Hire and operation of inflatable volleyball game.
Equipment: Inflatable court, blower, stakes/sandbags, volleyball.
	Hazard
	Persons at Risk
	Potential Harm
	Control Measures
	Risk

	Manual handling
	Staff
	Strains
	Team lift/trolley
	Low

	Inflatable movement
	Users
	Impact/injury
	Anchor securely; inspect anchors
	Low

	Electrical blower
	Staff/Public
	Shock
	PAT tested, RCD, cables covered
	Low

	Trips on entrance/cables
	Users
	Falls
	Clear access; cable covers
	Low

	Falls/collisions
	Players
	Bruises/sprains
	Limit numbers; supervise
	Medium

	Horseplay
	Players
	Injury
	No climbing/rough play
	Medium

	High winds/outdoor
	All
	Instability
	Follow wind limits; deflate if unsafe
	Low

	Damaged inflatable
	Users
	Injury
	Inspect before use
	Low

	Fire exits blocked
	Public
	Evacuation delay
	Keep escape routes clear
	Low


Additional Controls
Continuous adult supervision.
Suitable footwear or barefoot as instructed.
No sharp objects, food or drink.
Stop use during adverse weather.
Emergency Procedures
Stop play immediately if equipment becomes unsafe. Isolate blower power if required, administer first aid, record incidents and remove defective equipment from service.
