Risk Assessment – Spot On Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, supervised operation and dismantling of an indoor archery stall using low-poundage bows and suction-cup or foam safety arrows for temporary hire at events.
Persons at Risk
Staff, hirers, operators, participants, spectators and members of the public.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use safe lifting techniques and team lifts where required; use suitable handling equipment for heavier sections.
	Low

	Participant struck by game component
	Participants/Spectators
	Medium
	Keep the operating area controlled; provide clear instructions; prevent throwing or misuse; supervise continuously.
	Low

	Finger or hand trapping at controls
	Participants
	Medium
	Use the game only as designed; keep hands clear of gaps and edges; inspect controls before use.
	Low

	Electrical equipment / cable hazard
	Participants/Staff
	Medium
	Inspect power supply, plug and cables before use; route cables safely away from walkways; isolate defects.
	Low

	Trips around equipment and cables
	All
	Medium
	Keep floors clear of bags, cables and equipment; route cables away from pedestrian routes.
	Low

	Damaged game, controls or frame
	All
	Medium
	Inspect the unit before each session; remove damaged or defective equipment from use.
	Low

	Incorrect use / deliberate misuse
	Participants
	Medium
	Give a clear demonstration and safety briefing; prohibit climbing, striking or tampering; stop unsafe behaviour.
	Low

	Participant collision while playing
	Participants
	Medium
	Control player numbers; maintain adequate space around the game; supervise movement and queues.
	Low

	Overcrowding around game
	Participants/Spectators
	Medium
	Control player numbers and queues; maintain a clear area around the unit; supervise waiting participants.
	Low

	Spectators interfering with play
	Public
	Medium
	Define the play area and keep spectators clear of controls and operating positions where necessary.
	Low

	Slips or falls
	All
	Medium
	Operate on a clean, dry and level surface; keep surrounding floor clear of loose objects and trip hazards.
	Low

	Poor lighting / visibility
	Participants/Staff
	Medium
	Provide adequate ambient lighting so the game, controls, cables and surrounding hazards are clearly visible.
	Low

	Unsuitable participant age / ability
	Participants
	Medium
	Follow manufacturer guidance where available; provide clear instructions and appropriate supervision, particularly for younger users.
	Low

	Competitive or unsafe participant behaviour
	Participants
	Medium
	Set clear rules before play; prohibit pushing, striking equipment or unsafe behaviour; stop play if required.
	Low

	Unauthorised access to operating area
	Spectators/Public
	Medium
	Clearly define the operating area and control access so spectators do not interfere with participants or equipment.
	Low


Operational Controls
 Set up on a suitable, level surface with adequate space around the Spot On game.
 Give participants a clear safety briefing covering safe operation and correct use of the game.
 Use the game only as designed and prevent participants from climbing, striking or tampering with the unit.
 Maintain appropriate supervision, particularly where young children are participating.
 Stop activity immediately if unsafe behaviour, equipment faults, damaged components or unsafe conditions occur.
Emergency Procedures
 Stop the Spot On game immediately following any incident.
 Provide first aid where required and contact emergency services if necessary.
 Isolate damaged or defective equipment and prevent further use.
 Record all accidents and near misses.
Inspection Checklist
 Game frame and housing free from damage.
 Controls and operating surfaces secure and functioning correctly.
 Lights, displays or electronic components operate correctly where fitted.
 Electrical supply, plug and cables free from visible damage where applicable.
 Unit stable and securely positioned.
Training Requirements
 Staff trained in safe Spot On operation, manual handling, customer briefing, participant supervision, emergency procedures and equipment inspection.







