Risk Assessment – Driving Simulator Hire 
Activity Description
Transport, installation, operation, supervision and dismantling of driving simulators for events.
Persons at Risk
Participants, children, adults, operators, installation staff, spectators, organisers and the public.
Detailed Risk Assessment
	Hazard
	Persons
	Initial
	Control Measures
	Residual

	Manual handling
	Staff
	High
	Team lifting and trolleys
	Low

	Electrical shock
	All
	High
	PAT tested equipment and RCD protection
	Low

	Trip hazards
	All
	High
	Cable covers and cable management
	Low

	Frame instability
	Users
	High
	Level setup and bolt inspections
	Low

	Monitor falling
	Users
	High
	Secure stands and mounts
	Low

	Motion sickness
	Users
	Medium
	Warnings and stop if unwell
	Low

	Entrapment
	Users
	Medium
	Keep hands clear; supervise
	Low

	Fire
	All
	High
	Electrical inspection and emergency procedures
	Low


Operational Controls
Inspect frame, seat, steering, pedals, monitor, cables, PAT labels, RCD and software before opening.
Emergency Procedures
Stop activity, isolate power if safe, evacuate, administer first aid and contact emergency services where necessary.
Training
Manual handling, electrical safety, customer briefing, emergency procedures, first aid awareness.
