Risk Assessment – Giant Operation Hire
Activity Description
Transport, installation, operation and dismantling of a Giant Operation game for events.
Persons at Risk
Participants, staff, spectators and the public.

	Hazard
	Persons
	Initial
	Control Measures
	Residual

	Manual handling
	Staff
	High
	Team lifting
	Low

	Electrical fault
	All
	High
	PAT tested equipment; inspect before use
	Low

	Trip hazards
	All
	Medium
	Manage cables and keep area clear
	Low

	Pinch points
	Players
	Low
	Use as intended under supervision
	Low

	Player collisions
	Players
	Medium
	Queue management
	Low

	Equipment damage
	All
	Medium
	Pre-use inspections
	Low

	Weather (outdoors)
	All
	High
	Protect equipment; suspend in severe weather
	Low

	Dismantling
	Staff
	Medium
	Disconnect power and use safe lifting
	Low


Inspection Checklist
Check cabinet, wiring, probes, buzzer, power supply, PAT label, cables and cleanliness before use.
