Risk Assessment – Golf Swing Simulator Hire (HSE/AAIAC Style)
Activity Description
Assessment covers transport, installation, operation and dismantling of a portable golf swing simulator.
Persons at Risk
Participants, operators, spectators, staff and members of the public.
Detailed Risk Assessment
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling
	Staff
	High
	Team lift/use trolley
	Low

	Uneven ground
	Everyone
	High
	Level surface only
	Low

	Trailing cables
	Everyone
	Medium
	Cable covers and tidy routing
	Low

	Electrical equipment
	Everyone
	High
	PAT tested, RCD protection
	Low

	Golf club striking person
	Users/Public
	High
	Barrier and exclusion zone
	Low

	Golf ball rebound
	Users
	High
	Use impact screen and approved balls
	Low

	Screen/frame failure
	Everyone
	High
	Pre-use inspection
	Low

	Poor supervision
	Users
	Medium
	Operator present throughout
	Low

	Fire
	Everyone
	Medium
	Electrical inspections and evacuation
	Low

	Dismantling
	Staff
	Medium
	Power off and safe manual handling
	Low


Operational Controls
Inspect simulator, screen, frame, projector, launch monitor, cables, barriers and signage before use.
Emergency Procedures
Stop activity, isolate power, administer first aid, remove faulty equipment and follow site emergency procedures.
Inspection Checklist
Frame, impact screen, clubs, balls, projector, launch monitor, cables, RCD, barriers and signage.
Training Requirements
Manual handling, setup, electrical safety, safe operation, emergency procedures and daily inspections.
