Risk Assessment – Roll-a-Ball Derby Hire (HSE/AAIAC Style)
Activity Description
Delivery, setup, operation and collection of a Roll-a-Ball Derby fairground game for temporary hire at events.
Persons at Risk
Staff, hirers, participants, children and spectators.
	Hazard
	Persons at Risk
	Initial Risk
	Control Measures
	Residual Risk

	Manual handling during setup
	Staff
	Medium
	Use correct lifting techniques and team lifts where required.
	Low

	Trips around game
	All
	Medium
	Keep the playing area clear of loose balls and other obstructions.
	Low

	Balls leaving the game area
	Participants/Spectators
	Medium
	Use side barriers where fitted and supervise play.
	Low

	Player collisions
	Participants
	Medium
	Allow only one player per lane and maintain adequate spacing.
	Low

	Unstable equipment
	All
	Medium
	Position on firm, level ground and inspect before use.
	Low

	Damaged equipment
	All
	Low
	Inspect before hire and after collection; remove defective equipment from service.
	Low


Operational Controls
Set up on a firm, level surface.
Ensure all components are securely assembled.
Only one participant per lane at any time.
Collect stray balls regularly.
Withdraw damaged equipment from use immediately.
Emergency Procedures
Stop play if the game becomes unstable or unsafe.
Provide first aid where required.
Record and report all accidents and near misses.
Inspection Checklist
Frame secure.
Playing lanes undamaged.
Balls in good condition.
Area free from trip hazards.
Equipment complete and clean.
Training Requirements
Staff trained in manual handling, setup, inspection and customer safety briefing.
